{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":9,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["校园盲区安装照明灯具项目清单"]
[{"$nulls":7},"单位：元"]
["序号","项目名称","单位","参数","参考图片","数量","综合\n单价","金额","备注"]
[1,"校园照明盲区庭院灯","盏","\n规格:市电款  LED光源30W，防护等级P653.灯杆材质、规格:金属灯杆，H=3.5m, 尺寸:130*85mm，壁厚1.2mm",null,40,null,null,"含安装，不含地笼与水泥基础浇筑。\n\n以双方最终确认的样式为准。"]
[2,"孔德学区安装太阳能壁灯（60W）","盏","太阳能板6v 尺寸800*670.锂电池60AH 3.2v，LED光源60瓦，续航可持续三个阴雨天",null,10,null,null,"含安装"]
[3,"学益学区安装太阳能壁灯（60W）","盏","太阳能板800*670.锂电池60AH，LED光源60瓦",null,10,null,null,"含安装"]
[null,"合计"]