{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":7,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["暑期地瓷砖及道牙和树坑框维修工程量清单"]
[{"$nulls":6},"单位：元"]
["序号","项目名称","规格及做法","单位","数量","综合\n单价","金额"]
[1,"地瓷砖维修","瓷砖规格：60*60cm；做法：拆除空鼓瓷砖，拆除原有粘接层，铺贴新地瓷砖。\n位置：各楼宇地瓷砖零散脱落、空鼓处\n说明：瓷砖由学校提供。","m2",400]
[2,"道路道牙维修","做法：清理损坏的道牙面层，抹细石混凝土（掺胶浆）进行修复。","m",400]
[3,"树坑边框维修","树坑尺寸1.6m*1.6m。做法：\n拆除原有损坏的道牙边框，安装高20cm*厚10cm专用混凝土树坑框，修复树坑周边方砖（每个树坑周边方砖按2平米计算）。\n位置：男生公寓区","个",19]
[null,"小计"]