{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[[0,0,0,7],[3,1,11,1],[3,7,9,7]],"flags":["formulas_cached_only"]}
["宁夏育才中学校园内铺设方砖及人行道等维修采购项目清单"]
[{"$nulls":7},"单位：元"]
["序号","项目内容","位置","规格","数量","综合\n单价","金额","备   注"]
[1,"铺设方砖\n\n人行道","文化交流中心北边绿地内","30m*3m",90,null,null,"1-7项做法：\n原土夯实，\n15cm厚砂石料，\n3cm砂浆结合层，\n6cm厚20cm*20cm方砖。\n与绿地接触边栽道牙，长度约200米。\n\n\n\n\n\n"]
[2,null,"勤行多功能厅东南角绿地内","21m*4m",84]
[3,null,"勤行D教学楼东头绿地内","18m*4m",72]
[4,null,"勤行A教学楼西门口绿地","20m*3.5m",70]
[5,null,"小二楼西边小块空地","16.8m*9.7m",162.96]
[6,null,"孔德行政楼南边树坑","4.8m*2.8m*4个",53.76]
[7,null,"学益行政楼南边树坑","4.8m*2.8m*4个",53.76]
[8,null,"勤行入口处地砖更新","8m*10m",80,null,null,"将原砖清除，重新铺贴新砖"]
[9,null,"混凝土道牙","延长米",200]
[null,"小   计",{"$nulls":4},0]
[10,"混凝土路面井体维修",null,null,10,null,0,"将井口周边砼拆除，更换承重金属井盖，重新浇筑砼。"]
[null,"合   计",{"$nulls":4},0,"据实结算"]